|  |
| --- |
| **CRS sheet** |

|  |  |  |
| --- | --- | --- |
| **Requirement ID** | **Customer Requirement**  **(description of the customer requirements)** | **Date Received** |
| CRS-00-1 | Increase the air condition temperature | 5-3-2016 |
| CRS-00-2 | Decrease the air condition temperature | 5-3-2016 |
| CRS-00-3 | Increase the air condition Fan speed | 5-3-2016 |
| CRS-00-4 | Decrease the air condition Fan speed | 5-3-2016 |
| CRS-00-5 | Turn on the Air condition | 5-3-2016 |
| CRS-00-6 | Turn off the Air condition | 5-3-2016 |

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

|  |
| --- |
| **SIQ sheet** |

|  |  |  |  |
| --- | --- | --- | --- |
| **Requirement ID** | **Questionnaire** | **Customer Answer** | **Date Received** |
| SIQ-00-1 | LCD Size | Customer needs the cheapest LCD and acceptable size | 12-3-2016 |
| SIQ-01-2 | Push Button type | Tactile Switch | 12-3-2016 |
| SIQ-02-3 | Push Button functionality | 1- Selection Button  2-Increase Button  3-Decrease Button  4-On/Off Button | 12-3-2016 |
| SIQ-03-4 | Fan speed and Temperature | Configurable | 12-3-2016 |
| SIQ-04-5 | Default value when making reset | Latest Reading | 12-3-2016 |